%Schriftgröße, Layout, Papierformat, Art des Dokumentes
\documentclass[10pt,oneside,a4paper]{scrartcl}

%Einstellungen der Seitenränder
\usepackage[left=2cm,right=2cm,top=1.5cm,bottom=1.5cm,includeheadfoot]{geometry}

%neue Rechtschreibung
\usepackage[ngerman]{babel}

%Umlaute ermöglichen
\usepackage[utf8]{inputenc}

%Gesamtseitenzahl
\usepackage{lastpage}

% Kopf- und Fußzeile
% \usepackage[automark]{scrpage2} deprecated
\usepackage[automark]{scrlayer-scrpage}

%Quellcode-Listings
\usepackage{listings}

%Hyperlinks
\usepackage{hyperref}

% \text{}
\usepackage{amsmath}

%multi-row
\usepackage{multirow}

\usepackage{array}

%Kopfzeile
\ihead{CCNA v7.02: SRW (Switching, Routing, and Wireless Essentials)}
\chead{}
\ohead{kohnlehome.de/cisco/CCNA-2-15.pdf}
\setheadsepline{0.5pt}

%Fußzeile
\setfootsepline{0.5pt}
\ifoot{Franz Kohnle}
\cfoot{Seite \thepage\ von  \pageref{LastPage}}
\ofoot{\today}

\pagestyle{scrheadings}

\begin{document}

% Überschrift 
\begin{center}
    \LARGE % Schriftgröße
    \bfseries % Fettdruck
    \sffamily % Serifenlose Schrift
    15 IP Static Routing
\end{center}

\section*{15.1 Static Routes}
\begin{itemize}
    \item \texttt{Router(config)\# ip route network-address subnet-mask \{ ip-address | exit-intf [ip-address]\} [distance]}
    \item \texttt{Router(config)\# ipv6 route ipv6-prefix/prefix-length \{ipv6-address | exit-intf [ipv6-address]\} [distance]}
\end{itemize}

\section*{15.2 Configure IP Static Routes}
\begin{itemize}
    \item IPv4 / IPv6 Next-Hop Static Route
    \item IPv4 / IPv6 Directly Connected Static Route (mit Exit-Interface)
    \item IPv4 / IPv6 Fully Specified Static Route (Exit-Interface + Next Hop) (z.B. für link-local Next Hop)
\end{itemize}

\subsection*{Diagnose}
\begin{itemize}
    \item \texttt{show ip route}, \texttt{show ipv6 route}
    \item \texttt{show running-config}
\end{itemize}

\section*{15.3 Configure IP Default Static Routes}
\begin{itemize}
    \item \texttt{Router(config)\# ip route 0.0.0.0 0.0.0.0 \{ip-address | exit-intf\}}
    \item \texttt{Router(config)\# ipv6 route ::/0 \{ipv6-address | exit-intf\}}
\end{itemize}

\section*{15.4 Configure Floating Static Routes}
Backup-Routen mit Administrativer Distanz $> 1$
\begin{verbatim}
R1(config)# ip route 0.0.0.0 0.0.0.0 172.16.2.2
R1(config)# ip route 0.0.0.0 0.0.0.0 10.10.10.2 5
R1(config)# ipv6 route ::/0 2001:db8:acad:2::2
R1(config)# ipv6 route ::/0 2001:db8:feed:10::2 5    
\end{verbatim}

\section*{15.5 Configure Static Host Routes}
Zielnetz /32 bzw /128, z.B. für Route zu einem Server 

\section*{15.6.1 Packet Tracer - Configure IPv4 and IPv6 Static and Default Routes}

\end{document}
